### Weaving a binary

### encoded strap.

Cut along the dotted lines, then, using the ASCII character set, weave your name into the slots in binary code using slips of coloured paper. Pass the coloured paper under the white paper for a 0 and over the white paper for a 1.

A black screen with white dots

Description automatically generatedA black screen with white dots

Description automatically generatedHere I have woven DSH:

D = 01000100­­­

S = 01010011

H = 01001000

